Simulated wave averaged turbulence energy (dotted line), bore averaged turbulence energy (dashed line) and near-bed bore averaged turbulence energy (solid line) as function of cross-shore position.