Measured (thick dashed line) and simulated (thick solid line) test av-eraged sediment transport from bed level changes. The simulated transport is separated in a transport due to avalanching (dashed-dotted line) and a transport related to the hydrody-namics (dotted line).