Simulated test and depth averaged sediment concentration (solid line) compared with the sediment concentrations obtained from suction tubes (squares).